Toyota bZ4X – Specifications



|  |  |  |
| --- | --- | --- |
| **DRIVETRAIN** | **FWD** | **AWD** |
| TYPE | AC SYNCHRONOUS ELECTRIC GENERATOR |
| TOTAL POWER OUTPUT (DIN HP / kW) | 204 / 150 | 218 / 160 |
| FRONT MOTOR OUTPUT (DIN HP / kW) | 204 / 150 | 109 / 80 |
| REAR MOTOR OUTPUT (DIN HP / kW) | N/A | 109 / 80 |
| TORQUE (Nm) | 266 | 337 |

|  |  |
| --- | --- |
| **EV SYSTEM** |  |
| BATTERY | LITHIUM-ION |
| NUMBER OF CELLS | 96 |
| RATED VOLTAGE (V) | 355 |
| BATTERY CAPACITY (kWh) | 71.4 |

|  |  |  |
| --- | --- | --- |
| **PERFORMANCE** | **FWD** | **AWD** |
| MAX. SPEED (km/h) | 160 | 160 |
| ACC. 0-100 km/h (SEC) | 7.5 | 6.9 |
| BRAKE TYPE (FRONT & REAR) | VENTILATED DISC BRAKE |

|  |  |  |
| --- | --- | --- |
| **ENERGY CONSUMPTION (Wh/100km)** | **FWD** | **AWD** |
| WLTP CYCLE | from 1.43 | From 1.59 |

|  |  |  |
| --- | --- | --- |
| **RANGE (km)** | **FWD** | **AWD** |
| WLTP CYCLE (18” WHEELS) | 516 | 470 |
| WLTP CYCLE (20” WHEELS) | 436 | **411** |

|  |  |
| --- | --- |
| **EXTERIOR DIMENSIONS (mm)** |  |
| OVERALL LENGTH | 4,690 |
| OVERALL WIDTH | 1,860 |
| OVERALL HEIGHT | 1,650 |
| WHEELBASE | 2,850 |
| TRACK (FRONT/REAR) | 1,600/1,610 |
| MIN. RUNNING GROUND CLEARANCE | 177 (with 1 passenger) |
| TURNING RADIUS (TIRE/BODY) | 5.6 / 6.1 |
| TIRE SIZE (18”/20”) | 235/60R18 / 235/50R20 |
| WHEEL SIZE (18”/20”) | 18x7.5 / 20x7.5 |

|  |  |
| --- | --- |
| **INTERIOR DIMENSIONS (mm)** |  |
| LENGTH | 1,940 |
| WIDTH | 1,515 |
| HEIGHT | 1,160 (1,145 panoramic roof) |

|  |  |
| --- | --- |
| **CARGO (VDA)　(cm3)** |  |
| CAPACITY (INCLUDING UNDER DECK BOARD) | 452 (441 with subwoofer) |
| CAPACITY (SEATS DOWN UP TO ROOF) | **TBC** |

|  |  |  |
| --- | --- | --- |
| **WEIGHT(kg)** | **FWD** | **AWD** |
| TOWING CAPACITY | **750** | **750** |
| CURB WEIGHT | 1,895-1,980 | 1,985 – 2,065 |
| GVM | 2,465 | 2,550 |